|  |
| --- |
| **FORM 4 (Rule 5)** |
| **Section 8 of Care of Cathedrals Measure 2011** |
| **Public Notice on application to the Fabric Advisory Committee**  **PUBLIC NOTICE**  **TAKE NOTICE that the Chapter of the Cathedral Church of:**  Christ and the Blessed Virgin of Worcester |

1 February 2022

**has on this date:**

**applied to the Fabric Advisory Committee of the said cathedral for approval of the following proposal:**

A programme of works following damage caused by Storm Arwen of a fallen pinnacle and subsequent repairs

**Summary of the nature of work and its extent (and materials) [or in the case of an object, a short description of it and details of the proposal]**

ROOF COVERINGS AND RAINWATER GOODS:

* North Quire Aisle, recovering part of slate roof, repair to timber structure including replacement section of purlin.
* North Quire Aisle, local repairs to slate roof covering.
* Quire, north slope, local repairs to the slate roof covering.
* North Transept, east slope, local repairs to the roof covering.
* Quire, north parapet gutter, to rebuild and recover one bay of lead gutter.
* Quire and North Quire Aisle, north walls, to repair / replace rainwater goods and overhaul / repair locally parapet gutters.

STONEWORK REPAIRS:

* North Quire Aisle, local repairs, repointing and replacement of stone.
* Quire, north wall, local repairs, repointing and replacement of stone.
* Tower, northeast corner, upper pinnacles to corner buttress, to dismantle and rebuild incorporating new carved stone, stainless steel cramps and rod.
* Tower, northeast corner, local repairs and repointing to stonework.

MECHANICAL & ELECTRICAL SERVICES, NORTH QUIRE AISLE ROOF VOID:

* Cathedral Heating System, to repair system as existing.
* Electrical System, to replace local lighting and power provision, all to be in accordance with current regulations.
* Fire Detection System, to repair system as existing.
* Organ, specialist electric equipment, to replace ‘like for like’.
* Organ, heating / cooling equipment, to replace existing with specification of equipment installed within the organ chamber of the South Quire Aisle.

SPECIALIST CLEANING:

* Quire Organ, by Nicholson & Co
* Monument, No 131, Randolph Marriott (1807)
* Monument, No 132, Bishop Isaac Maddox (132)
* East End of Cathedral, all fabric, furniture, and fittings.

All works to be carried out in accordance with Worcester Cathedral Conservation Plan Polices, refer to report R16A – 14\_083, July 2017 and the Specification, Schedule of Works and Drawings, Report R3 – 21\_115.

ITEMS FOR FURTHER CONSIDERATION, DISCUSSION AND APPROVAL BY THE FAC AT A LATER DATE:

* Repair to the vaulting of the North Quire Aisle
* Repairs to the Detailed design of three grotesques / beasts to the pinnacle, a philosophy and maquettes for each design will be provided for consideration.
* Repairs to Monument 131 and Monument 132 within the North Quire Aisle, if required.
* Further repairs to the Tower.

**Plans, drawings, specifications or other documents**

**Copies of the plans, drawings, specification and other documents accompanying this application may be examined at the office of the Chapter of the Cathedral Church**

*Insert address and contact details*

By request with Val Floy, Chief Operating Officer

8 College Yard, Worcester, WR1 2LA

[valfloy@worcestercathedral.org.uk](mailto:valfloy@worcestercathedral.org.uk)

01905 732907

12 noon and 3pm

**Between the hours of:**

1 February 2022

**From this day:**

**and until:**

28 February 2022

**REPRESENTATIONS**

**If you wish to make representations about the whole or any part of the proposal described in this Notice you should write to the Secretary of the Fabric Advisory Committee:** *insert postal and email address.*

Rob Alexander

c/o 8 College Yard

Worcester

WR1 2LA

|  |
| --- |
| **So that it reaches the Secretary not later than:** *insert a date ending 28 days after the time of the commencement of the period for representations.*  28 February 2022 |